**Dualcopter mixer values for KK 2 flyghtcontrol**

**Pgain=30 Plim.=100 Igain=0 Plim.=0**

**Roll CH1 Pitch CH2 Throttle CH3 Yaw CH4**

**CH THR AIL ELEV RUD OFFS TYPE RATE**

**CH1 100 100 0 0 0 ESC HIGH**

**CH2 100 100 0 0 0 ESC HIGH**

**CH3 0 0 100 -100 50 SERVO LOW**

**CH4 0 0 -100 -100 50 SERVO LOW**